;
; AMI - The Asterisk Manager Interface
; 
; Third party application call management support
; and PBX event supervision
;
; This configuration file is read every time someone
; logs in
;
; Use the "show manager commands" at the CLI to list
; availabale manager commands and their authorization
; levels.
;
; "show manager command <command>" will show a help text.
;
; ------------------- SECURITY NOTE -----------------
; Note that you should not enable the AMI on a public
; IP address. If needed, block this TCP port with
; iptables (or another FW software) and reach it
; with IPsec, SSH or SSL vpn tunnel
;
[general]
enabled = no
port = 5038
bindaddr = 0.0.0.0
;displayconnects = yes

;[mark]
;secret = mysecret
;deny=0.0.0.0/0.0.0.0
;permit=209.16.236.73/255.255.255.0
;
; Authorization for various classes 
;read = system,call,log,verbose,command,agent,user
;write = system,call,log,verbose,command,agent,user
