;
; alarmreceiver.conf
;
; Sample configuration file for the Asterisk alarm receiver application.
;


[general]

;                                                                                                                                   
; Specify a timestamp format for the metadata section of the event files
; Default is %a %b %d, %Y @ %H:%M:%S %Z
	        
timestampformat = %a %b %d, %Y @ %H:%M:%S %Z

;
; Specify a command to execute when the caller hangs up
;
; Default is none
;

;eventcmd = yourprogram -yourargs ...

;
; Specify a spool directory for the event files. This setting is required if you want the app to be useful.
; Event files written to the spool directory will be of the template event-XXXXXX, where XXXXXX is a random
; and unique alphanumeric string.
;
; Default is none, and the events will be dropped on the floor.
;

eventspooldir = /tmp

; 
; The alarmreceiver app can either log the events one-at-a-time to individual files in the spool 
; directory, or it can store them until the caller disconnects and write them all to one file.
;
; The default setting for logindividualevents is no.
;

logindividualevents = no

;
; The timeout for receiving the first DTMF digit is adjustable from  1000 msec. to 10000 msec. The
; default is 2000 msec. Note: if you wish to test the receiver by entering digits manually, set this
; to a reasonable time out like 10000 milliseconds. 

fdtimeout = 2000

;
; The timeout for receiving subsequent DTMF digits is adjustable from  110 msec. to 4000 msec. The
; default is 200 msec. Note: if you wish to test the receiver by entering digits manually, set this
; to a reasonable time out like 4000 milliseconds. 
;

sdtimeout = 200

;
; The loudness of the ACK and Kissoff tones is adjustable from 100 to 8192. The default is 8192
; This shouldn't need to be messed with, but is included just in case there are problems with 
; signal levels.
;

loudness = 8192

;
; The db-family setting allows the user to capture statistics on the number of calls, and the errors
; the alarm receiver sees. The default is for no db-family name to be defined and the database logging
; to be turned off.
;

;db-family = yourfamily:

;
; End of alarmreceiver.conf
;
